{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["汇总表","综合单价报价表"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"汇总表","index":0,"n_rows":10,"n_cols":5,"rows_kept":10,"merged":[[0,0,0,4],[9,0,9,4]],"flags":["formulas_cached_only"]}
["投标报价汇总表"]
["序号","名    称","规格型号","总价(元) ","备  注"]
[1,"气箱脉冲布袋除尘器"]
[2,"气箱脉冲布袋除尘器"]
[3,"阀门控制部分"]
[4,"HMC80单机移位安装","反击破移至振动筛"]
[5,"干雾抑尘系统"]
[6,"其他"]
[null,"合计",null,0]
["注：投标内容为气箱脉冲布袋除尘器、阀门、干雾抑尘系统等设备采购、安装、调试、验收；报价包含人工费、材料费、设备费、机械费、规费、措施费、管理费、利润、施工期间的成品保护、安全责任、文明施工、调试费及验收、9%税费等所有费用。"]

{"sheet":"综合单价报价表","index":1,"n_rows":71,"n_cols":9,"rows_kept":71,"merged":[[0,0,0,8]],"flags":["formulas_cached_only"]}
["设备采购及安装综合单价报价表"]
["序号","分项名称","型号规格","单位","数量","综合单价(元)","总价(元)","推荐品牌","投标品牌"]
["一","气箱脉冲布袋除尘器","PPCS96-5"]
[1,"除尘器壳体","壳体δ5mm,花板δ8mm","吨",14,null,0]
[2,"布袋","Φ130×3060mm涤纶针刺毡","条",480,null,0]
[3,"骨架","Φ125×3010mm镀锌","件",480,null,0]
[4,"脉冲阀","3寸直角式","套",5,null,0]
[5,"提升阀气缸","SC100×300-FA","套",5,null,0]
[6,"提升阀","Φ750mm","套",5,null,0]
[7,"电磁换向阀","DC24V","套",5,null,0]
[8,"气管","Φ89-Φ108","套",1,null,0]
[11,"气包","Φ630×1000mm","个",1,null,0]
[12,"气源三联件","QFLJW-L40/L25","个",2,null,0]
[13,"重锤翻板阀","300×300mm","台",5,null,0]
[14,"气路系统",null,"套",1,null,0]
[15,"电路系统","电缆、桥架","套",1,null,0]
[16,"脉冲控制仪",null,"台套",1,null,0]
[17,"风机、电机","G6-51NO9D-37KW","台套",1,null,0]
[18,"变频器","45KW","套",1,null,0]
[null,"小计",{"$nulls":4},0]
["二","气箱脉冲布袋除尘器（含设备基础）","PPCS128-12"]
[1,"除尘器壳体","壳体δ5mm,花板δ8mm","吨",47.5,null,0]
[2,"布袋","Φ130×3060mm涤纶针刺毡","条",1536,null,0]
[3,"骨架","Φ125×3010mm镀锌","件",1536,null,0]
[4,"脉冲阀","3寸直角式","套",24,null,0]
[5,"提升阀气缸","SC100×300-FA","套",12,null,0]
[6,"提升阀","Φ750mm","套",12,null,0]
[7,"电磁换向阀","DC24V","套",12,null,0]
[8,"气管","Φ89-Φ108","套",2,null,0]
[9,"储气罐","1m³/0.8MPa","套",1,null,0]
[10,"螺杆空压机","3m³/min","台",1,null,0]
[11,"气包","Φ630×1000mm","个",2,null,0]
[12,"气源三联件","QFLJW-L40/L25","个",2,null,0]
[13,"重锤翻板阀","300×300mm","台",6,null,0]
[14,"气路系统",null,"套",1,null,0]
[15,"电路系统","电缆、桥架","套",1,null,0]
[16,"PLC控制柜（控制3台HMC80除尘器）","PLC-200系列","台套",1,null,0]
[17,"风机、电机","G4-68NO11.5D-4-110KW","台套",1,null,0]
[18,"变频器","132KW","套",1,null,0]
[19,"螺旋输送器","GX300×20000","台套",1,null,0]
[null,"小计",{"$nulls":4},0]
["三","阀门控制部分"]
[1,"手动阀门","Φ540","个",4,null,0,"鄂式破碎机入口、1号振动筛筛顶、2号振动筛筛顶、3号振动筛筛顶"]
[2,"手动阀门","Φ400","个",1,null,0,"反击破入口"]
[3,"手动阀门","Φ325","个",1,null,0,"反击破出口"]
[4,"手动阀门","Φ273","个",5,null,0,"鄂式破碎机下料口、渣土外运皮带受料口、3号振动筛下料（3个）"]
[null,"小计",{"$nulls":4},0]
["四","除尘器移位安装"]
[null,"移位安装费","HMC80","套",1,8000]
[null,"小计",{"$nulls":4},0]
["五","干雾抑尘系统"]
[1,"干雾炮机","GW2C/碳钢喷塑","台",2,null,0]
[2,"气雾喷射器","Q15C","台",4,null,0]
[3,"分控箱","GK2C","台",16,null,0]
[4,"万向节总成",null,"个",70,null,0]
[5,"超声波喷头",null,"个",150,null,0,"国标"]
[6,"空压机组","55KW,0.8MPa，储气罐1m³","台套",2,null,0]
[7,"电磁阀","DN25/黄铜先导阀","个",16,null,0]
[8,"电磁阀","DN15/黄铜先导阀","个",32,null,0]
[9,"液压管","DN15/1.6MPa/平口螺纹","批",1,null,0]
[10,"供水管道","DN50/热镀锌管","批",1,null,0]
[11,"供气管道","DN25/热镀锌管","批",1,null,0]
[12,"电缆桥架",null,"项",1,null,0]
[null,"小计",{"$nulls":4},0]
["六","其他"]
[1,"管道、烟罩及烟囱（15m）等非标",null,"吨",28,null,0,"据实结算、质量符合国标要求"]
[2,"铜芯电缆穿管安装","ZRYJV-0.6/1KV 4×185+1×70mm2","米",260,null,0,"据实结算"]
[3,"电缆头制作安装",null,"个",2,null,0]
[4,"水箱","10m3","座",2,null,0,"5mm钢板制作，含油漆"]
[null,"小计",{"$nulls":4},0]
[null,"合计",{"$nulls":4},0]